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Back Panel Connectors
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USB 10Gbps Type-A port (From XSTOE chipset)
+ Flash BIOS port

2| USB10Gbps Type-A port (From XSTOE chipset)

3| UsB 106bps Type- ports (From RTS5420)

Flash BIOS button - Please refer to page T3 for details about updating BIOS
with Flash BIOS button,

Clear CMOS button - Power offyour computer. Press and hold the Clear
CMOS button for about 5-10 seconds to reset BIOS to default values.

‘Smart button - there are 4 unctions for the smart button, Please refer o the

BI0S manual for details about selecting the smart button function.

* Reset (default) - press the smart button to reset the system.

+ Mystic Light ony off - press the smart button to turn on/ offall the
onboard LEDs. The Mystic Light on/ offfunction modeis unavailable

6 | when the LED_SwWA (EZ LED Control) switch turns OFF.

+ Safe Boot - press and hold the smart button while simultaneously
starting the system to enter Safe Boot mode. This will boot the system
with default settings and lower the PCle mode associated with the CPU.

+ Turbo Fan - pressing the smart button synchronizes the fan speed of all
fans. The fan speed can be synchronized to full speed or default speed.
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7| 256bps LAN(RI4S) port
8| 5Gbps LAN(RI45) port
9| WiFi antenna connectors
10| Lineoutport
11| Micinport
s 1L
15| USBA40GDpS Type-C ports (From ASHA242)
+ Supports DisplayPort over USB Type-
14| UsB 1065ps Type C port (rom CPU)
15 | USB 10Gbps Type A ports (From XETOE Chipset)
16| USB 10Gbps Type Aport (From CPU)
17| USB 106bps Type C port (From XETOE Chipset]
18| Optical /PDIF Out connector





